**Erosion and Sediment Control Plan**

Maintain an up-to-date site map. BMP location will change frequently as the work on a construction site progresses. Your permit requires that you keep your site map up to-date. Submit a site map with the location of these BMPs. Indicate the current location of the following:

|  |  |
| --- | --- |
| * Portable toilets must be on pervious surfaces.
 | * Chemicals on site.
 |
| * Washout containment for concrete washout water, paint, stucco.
 | * Stockpiles
* Material storage areas.
 |
| * Dumpsters or other trash and debris containers.
 | * Vehicle and equipment fueling
 |
| * Perimeter control & Stabilized
 | * Construction entrance/exit
 |



If a marked-up site map is too full to be easily read, you should date and fold it, put it in the SWPPP for documentation, and start a new one.